**EQUIPMENT SCHEDULE**

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| TAG no. | Quantity | Description | Brand/Model | Capacity | No. of Indoor units connected | Electrical Data | | | Remarks |
| V | ϕ | Hz |
| CH-1 | 1 | Air Cooled Chiller | Carrier/0700A | 668.1 kW | 96 | --- | --- | --- | See attached catalogue for equipment detailed specification |

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| TAG no. | Quantity | Description | Brand/Model | Capacity | No. of Indoor units connected | Electrical Data | | | Remarks |
| V | ϕ | Hz |
| AHU | 1 | 39G Air Handling Unit | Carrier/Y SM-B | 668.1 kW | 15 | --- | --- | --- | See attached catalogue for equipment detailed specification |

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| TAG no. | Quantity | Description | Brand/Model | Capacity (TOR) | Area Served | Electrical Data | | | Remarks |
| V | ϕ | Hz |
| FCU-A1 | 1 | Ceiling Casette Chilled Water Fan Coil Unit | Daikin/FWMJCC2BV1 | 1..5 | Supply Room | 230 | 60 | 1 | See attached catalogue for equipment detailed specification |
| FCU-A2 | 1 | Ceiling Casette Chilled Water Fan Coil Unit | Daikin/FWMJCC2BV1 | 1 | Maintenance Office | 230 | 60 | 1 | See attached catalogue for equipment detailed specification |
| FCU-A3 | 1 | Ceiling Casette Chilled Water Fan Coil Unit | Daikin/FWMJCC2BV1 | 1 | Pharmacy | 230 | 60 | 1 | See attached catalogue for equipment detailed specification |
| FCU-A4 | 1 | Ceiling Casette Chilled Water Fan Coil Unit | Daikin/FWMJCC2BV1 | 1 | Medical Record's Office | 230 | 60 | 1 | See attached catalogue for equipment detailed specification |
| FCU-A5 | 1 | Ceiling Casette Chilled Water Fan Coil Unit | Daikin/FWMJCC2BV1 | 1 | Medical Records | 230 | 60 | 1 | See attached catalogue for equipment detailed specification |
| FCU-A6 | 1 | Ceiling Casette Chilled Water Fan Coil Unit | Daikin/FWMJCC2BV1 | 1 | PHILHEALTH | 230 | 60 | 1 | See attached catalogue for equipment detailed specification |
| FCU-A7 | 1 | Ceiling Casette Chilled Water Fan Coil Unit | Daikin/FWMJCC2BV1 | 1 | Doctor's on Duty | 230 | 60 | 1 | See attached catalogue for equipment detailed specification |
| FCU-A8 | 1 | Ceiling Casette Chilled Water Fan Coil Unit | Daikin/FWMJCC2BV1 | 1 | OPD clinic dental 1 | 230 | 60 | 1 | See attached catalogue for equipment detailed specification |
| FCU-A9 | 1 | Ceiling Casette Chilled Water Fan Coil Unit | Daikin/FWMJCC2BV1 | 1 | OPD clinic dental 2 | 230 | 60 | 1 | See attached catalogue for equipment detailed specification |
| FCU-A10 | 1 | Ceiling Casette Chilled Water Fan Coil Unit | Daikin/FWMJCC2BV1 | 1 | OPD Clinic Pedia 1 | 230 | 60 | 1 | See attached catalogue for equipment detailed specification |
| FCU-A11 | 1 | Ceiling Casette Chilled Water Fan Coil Unit | Daikin/FWMJCC2BV1 | 1 | OPD Clinic Pedia 2 | 230 | 60 | 1 | See attached catalogue for equipment detailed specification |
| FCU-A12 | 1 | Ceiling Casette Chilled Water Fan Coil Unit | Daikin/FWMJCC2BV1 | 1 | Radiologist Office | 230 | 60 | 1 | See attached catalogue for equipment detailed specification |
| FCU-A13 | 1 | Ceiling Casette Chilled Water Fan Coil Unit | Daikin/FWMJCC2BV1 | 1 | Dark Room | 230 | 60 | 1 | See attached catalogue for equipment detailed specification |
| FCU-A14 | 1 | Ceiling Casette Chilled Water Fan Coil Unit | Daikin/FWMJCC2BV1 | 1 | X-ray Room | 230 | 60 | 1 | See attached catalogue for equipment detailed specification |
| FCU-A15 | 1 | Ceiling Casette Chilled Water Fan Coil Unit | Daikin/FWMJCC2BV1 | 1 | Linen Office | 230 | 60 | 1 | See attached catalogue for equipment detailed specification |
| FCU-A16 | 1 | Ceiling Casette Chilled Water Fan Coil Unit | Daikin/FWMJCC2BV1 | 2.5 | Cooking Area | 230 | 60 | 1 | See attached catalogue for equipment detailed specification |
| FCU-A17 | 1 | Ceiling Casette Chilled Water Fan Coil Unit | Daikin/FWMJCC2BV1 | 1 | Dietician's Office | 230 | 60 | 1 | See attached catalogue for equipment detailed specification |
| FCU-A18 | 2 | Ceiling Casette Chilled Water Fan Coil Unit | Daikin/FWMJCC2BV1 | 1.5 | Dietary | 230 | 60 | 1 | See attached catalogue for equipment detailed specification |
| FCU-A19 | 2 | Ceiling Casette Chilled Water Fan Coil Unit | Daikin/FWMJCC2BV1 | 1 | Staff Dining | 230 | 60 | 1 | See attached catalogue for equipment detailed specification |
| FCU-A20 | 1 | Ceiling Casette Chilled Water Fan Coil Unit | Daikin/FWMJCC2BV1 | 1.5 | Administrative Office | 230 | 60 | 1 | See attached catalogue for equipment detailed specification |
| FCU-A21 | 1 | Ceiling Casette Chilled Water Fan Coil Unit | Daikin/FWMJCC2BV1 | 1 | Social Welfare | 230 | 60 | 1 | See attached catalogue for equipment detailed specification |
| FCU-A22 | 1 | Ceiling Casette Chilled Water Fan Coil Unit | Daikin/FWMJCC2BV1 | 1 | Admin's Office | 230 | 60 | 1 | See attached catalogue for equipment detailed specification |
| FCU-A23 | 9 | Ceiling Casette Chilled Water Fan Coil Unit | Daikin/FWMJCC2BV1 | 1.5 | Canteen | 230 | 60 | 1 | See attached catalogue for equipment detailed specification |
| FCU-A24 | 1 | Ceiling Casette Chilled Water Fan Coil Unit | Daikin/FWMJCC2BV1 | 1 | OPD Clinic OB-gyne | 230 | 60 | 1 | See attached catalogue for equipment detailed specification |
| FCU-A25 | 1 | Ceiling Casette Chilled Water Fan Coil Unit | Daikin/FWMJCC2BV1 | 1 | Ultrasound | 230 | 60 | 1 | See attached catalogue for equipment detailed specification |
| FCU-A26 | 1 | Ceiling Casette Chilled Water Fan Coil Unit | Daikin/FWMJCC2BV1 | 1 | OPD Records | 230 | 60 | 1 | See attached catalogue for equipment detailed specification |
| FCU-A27 | 1 | Ceiling Casette Chilled Water Fan Coil Unit | Daikin/FWMJCC2BV1 | 1 | OPD info and admitting | 230 | 60 | 1 | See attached catalogue for equipment detailed specification |
| FCU-A28 | 1 | Ceiling Casette Chilled Water Fan Coil Unit | Daikin/FWMJCC2BV1 | 1 | Cashier | 230 | 60 | 1 | See attached catalogue for equipment detailed specification |
| FCU-A29 | 1 | Ceiling Casette Chilled Water Fan Coil Unit | Daikin/FWMJCC2BV1 | 1 | Billing | 230 | 60 | 1 | See attached catalogue for equipment detailed specification |
| FCU-A30 | 1 | Ceiling Casette Chilled Water Fan Coil Unit | Daikin/FWMJCC2BV1 | 1 | Admitting | 230 | 60 | 1 | See attached catalogue for equipment detailed specification |
| FCU-A31 | 1 | Ceiling Casette Chilled Water Fan Coil Unit | Daikin/FWMJCC2BV1 | 1 | OPD Clinic Medical 1 | 230 | 60 | 1 | See attached catalogue for equipment detailed specification |
| FCU-A32 | 1 | Ceiling Casette Chilled Water Fan Coil Unit | Daikin/FWMJCC2BV1 | 1 | OPD Clinic Medical 2 | 230 | 60 | 1 | See attached catalogue for equipment detailed specification |
| FCU-A33 | 1 | Ceiling Casette Chilled Water Fan Coil Unit | Daikin/FWMJCC2BV1 | 1 | OPD Clinic Surgery 1 | 230 | 60 | 1 | See attached catalogue for equipment detailed specification |
| FCU-A34 | 1 | Ceiling Casette Chilled Water Fan Coil Unit | Daikin/FWMJCC2BV1 | 1 | OPD Clinic Surgery 2 | 230 | 60 | 1 | See attached catalogue for equipment detailed specification |
| FCU-A35 | 1 | Ceiling Casette Chilled Water Fan Coil Unit | Daikin/FWMJCC2BV1 | 1 | OPD info and admitting | 230 | 60 | 1 | See attached catalogue for equipment detailed specification |
| FCU-A36 | 1 | Ceiling Casette Chilled Water Fan Coil Unit | Daikin/FWMJCC2BV1 | 1 | OPD Records | 230 | 60 | 1 | See attached catalogue for equipment detailed specification |

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| TAG no. | Quantity | Description | Brand/Model | Capacity (TOR) | Area Served | Electrical Data | | | Remarks |
| V | ϕ | Hz |
| FCU-B1 | 2 | Ceiling Casette Chilled Water Fan Coil Unit | Daikin/FWMJCC2BV1 | 2.5 | 5-Bed Ward 1 | 230 | 60 | 1 | See attached catalogue for equipment detailed specification |
| FCU-B2 | 2 | Ceiling Casette Chilled Water Fan Coil Unit | Daikin/FWMJCC2BV1 | 2.5 | 5-Bed Ward 2 | 230 | 60 | 1 | See attached catalogue for equipment detailed specification |
| FCU-B3 | 2 | Ceiling Casette Chilled Water Fan Coil Unit | Daikin/FWMJCC2BV1 | 2.5 | 5-Bed Ward 3 | 230 | 60 | 1 | See attached catalogue for equipment detailed specification |
| FCU-B4 | 2 | Ceiling Casette Chilled Water Fan Coil Unit | Daikin/FWMJCC2BV1 | 2.5 | 5-Bed Ward 4 | 230 | 60 | 1 | See attached catalogue for equipment detailed specification |
| FCU-B5 | 1 | Ceiling Casette Chilled Water Fan Coil Unit | Daikin/FWMJCC2BV1 | 1 | Private Room 1 | 230 | 60 | 1 | See attached catalogue for equipment detailed specification |
| FCU-B6 | 1 | Ceiling Casette Chilled Water Fan Coil Unit | Daikin/FWMJCC2BV1 | 1 | Private Room 2 | 230 | 60 | 1 | See attached catalogue for equipment detailed specification |
| FCU-B7 | 1 | Ceiling Casette Chilled Water Fan Coil Unit | Daikin/FWMJCC2BV1 | 2.5 | Chief Nurse | 230 | 60 | 1 | See attached catalogue for equipment detailed specification |
| FCU-B8 | 1 | Ceiling Casette Chilled Water Fan Coil Unit | Daikin/FWMJCC2BV1 | 1.5 | Treatment Room | 230 | 60 | 1 | See attached catalogue for equipment detailed specification |
| FCU-B9 | 1 | Ceiling Casette Chilled Water Fan Coil Unit | Daikin/FWMJCC2BV1 | 1 | Private Room 3 | 230 | 60 | 1 | See attached catalogue for equipment detailed specification |
| FCU-B10 | 1 | Ceiling Casette Chilled Water Fan Coil Unit | Daikin/FWMJCC2BV1 | 1 | Private Room 4 | 230 | 60 | 1 | See attached catalogue for equipment detailed specification |
| FCU-B11 | 1 | Ceiling Casette Chilled Water Fan Coil Unit | Daikin/FWMJCC2BV1 | 1 | Private Room 5 | 230 | 60 | 1 | See attached catalogue for equipment detailed specification |
| FCU-B12 | 1 | Ceiling Casette Chilled Water Fan Coil Unit | Daikin/FWMJCC2BV1 | 1 | Private Room 6 | 230 | 60 | 1 | See attached catalogue for equipment detailed specification |
| FCU-B13 | 1 | Ceiling Casette Chilled Water Fan Coil Unit | Daikin/FWMJCC2BV1 | 1 | Private Room 7 | 230 | 60 | 1 | See attached catalogue for equipment detailed specification |
| FCU-B14 | 1 | Ceiling Casette Chilled Water Fan Coil Unit | Daikin/FWMJCC2BV1 | 1 | Private Room 8 | 230 | 60 | 1 | See attached catalogue for equipment detailed specification |
| FCU-B15 | 1 | Ceiling Casette Chilled Water Fan Coil Unit | Daikin/FWMJCC2BV1 | 1 | Reception | 230 | 60 | 1 | See attached catalogue for equipment detailed specification |
| FCU-B16 | 2 | Ceiling Casette Chilled Water Fan Coil Unit | Daikin/FWMJCC2BV1 | 2 | Chief of Hospital | 230 | 60 | 1 | See attached catalogue for equipment detailed specification |
| FCU-B17 | 2 | Ceiling Casette Chilled Water Fan Coil Unit | Daikin/FWMJCC2BV1 | 2 | Conference Room | 230 | 60 | 1 | See attached catalogue for equipment detailed specification |
| FCU-B18 | 2 | Ceiling Casette Chilled Water Fan Coil Unit | Daikin/FWMJCC2BV1 | 2 | Chief of Clinics | 230 | 60 | 1 | See attached catalogue for equipment detailed specification |
| FCU-B19 | 1 | Ceiling Casette Chilled Water Fan Coil Unit | Daikin/FWMJCC2BV1 | 1 | 3-Bed Ward 1 | 230 | 60 | 1 | See attached catalogue for equipment detailed specification |
| FCU-B20 | 1 | Ceiling Casette Chilled Water Fan Coil Unit | Daikin/FWMJCC2BV1 | 2 | 3-Bed Ward 2 | 230 | 60 | 1 | See attached catalogue for equipment detailed specification |
| FCU-B21 | 1 | Ceiling Casette Chilled Water Fan Coil Unit | Daikin/FWMJCC2BV1 | 2 | 3-Bed Ward 3 | 230 | 60 | 1 | See attached catalogue for equipment detailed specification |
| FCU-B22 | 1 | Ceiling Casette Chilled Water Fan Coil Unit | Daikin/FWMJCC2BV1 | 1 | 3-Bed Ward 4 | 230 | 60 | 1 | See attached catalogue for equipment detailed specification |
| FCU-B23 | 1 | Ceiling Casette Chilled Water Fan Coil Unit | Daikin/FWMJCC2BV1 | 1 | CSSR | 230 | 60 | 1 | See attached catalogue for equipment detailed specification |
| FCU-B24 | 1 | Ceiling Casette Chilled Water Fan Coil Unit | Daikin/FWMJCC2BV1 | 1 | Autoclave Area | 230 | 60 | 1 | See attached catalogue for equipment detailed specification |
| FCU-B25 | 2 | Ceiling Casette Chilled Water Fan Coil Unit | Daikin/FWMJCC2BV1 | 2 | Sterile Room | 230 | 60 | 1 | See attached catalogue for equipment detailed specification |
| FCU-B26 | 2 | Ceiling Casette Chilled Water Fan Coil Unit | Daikin/FWMJCC2BV1 | 2 | Lounge Area | 230 | 60 | 1 | See attached catalogue for equipment detailed specification |
| FCU-B27 | 1 | Ceiling Casette Chilled Water Fan Coil Unit | Daikin/FWMJCC2BV1 | 1 | Pre-Mature Nursery | 230 | 60 | 1 | See attached catalogue for equipment detailed specification |
| FCU-B28 | 1 | Ceiling Casette Chilled Water Fan Coil Unit | Daikin/FWMJCC2BV1 | 1 | Pathologic Nursery | 230 | 60 | 1 | See attached catalogue for equipment detailed specification |
| FCU-B29 | 1 | Ceiling Casette Chilled Water Fan Coil Unit | Daikin/FWMJCC2BV1 | 1 | Anesthesia Office | 230 | 60 | 1 | See attached catalogue for equipment detailed specification |
| FCU-B30 | 1 | Ceiling Casette Chilled Water Fan Coil Unit | Daikin/FWMJCC2BV1 | 1 | Clean-up Room | 230 | 60 | 1 | See attached catalogue for equipment detailed specification |

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| TAG no. | Quantity | Description | Brand/Model | Capacity (TOR) | Area Served | Electrical Data | | | Remarks |
| V | ϕ | Hz |
| FCU-C1 | 2 | Ceiling Casette Chilled Water Fan Coil Unit | Daikin/FWMJCC2BV1 | 3 | 5- BedWard 1 | 230 | 60 | 1 | See attached catalogue for equipment detailed specification |
| FCU-C2 | 2 | Ceiling Casette Chilled Water Fan Coil Unit | Daikin/FWMJCC2BV1 | 3 | 5- BedWard 2 | 230 | 60 | 1 | See attached catalogue for equipment detailed specification |
| FCU-C3 | 1 | Ceiling Casette Chilled Water Fan Coil Unit | Daikin/FWMJCC2BV1 | 1.5 | Private Room 1 | 230 | 60 | 1 | See attached catalogue for equipment detailed specification |
| FCU-C4 | 1 | Ceiling Casette Chilled Water Fan Coil Unit | Daikin/FWMJCC2BV1 | 1.5 | Private Room 2 | 230 | 60 | 1 | See attached catalogue for equipment detailed specification |
| FCU-C5 | 1 | Ceiling Casette Chilled Water Fan Coil Unit | Daikin/FWMJCC2BV1 | 1.5 | Private Room 3 | 230 | 60 | 1 | See attached catalogue for equipment detailed specification |
| FCU-C6 | 1 | Ceiling Casette Chilled Water Fan Coil Unit | Daikin/FWMJCC2BV1 | 1.5 | Private Room 4 | 230 | 60 | 1 | See attached catalogue for equipment detailed specification |
| FCU-C7 | 1 | Ceiling Casette Chilled Water Fan Coil Unit | Daikin/FWMJCC2BV1 | 1.5 | Private Room 5 | 230 | 60 | 1 | See attached catalogue for equipment detailed specification |
| FCU-C8 | 1 | Ceiling Casette Chilled Water Fan Coil Unit | Daikin/FWMJCC2BV1 | 1.5 | Private Room 6 | 230 | 60 | 1 | See attached catalogue for equipment detailed specification |
| FCU-C9 | 1 | Ceiling Casette Chilled Water Fan Coil Unit | Daikin/FWMJCC2BV1 | 3 | Chief Nurse | 230 | 60 | 1 | See attached catalogue for equipment detailed specification |
| FCU-C10 | 1 | Ceiling Casette Chilled Water Fan Coil Unit | Daikin/FWMJCC2BV1 | 2.5 | 3- Bed Ward 1 | 230 | 60 | 1 | See attached catalogue for equipment detailed specification |
| FCU-C11 | 1 | Ceiling Casette Chilled Water Fan Coil Unit | Daikin/FWMJCC2BV1 | 1.5 | Private Room 7 | 230 | 60 | 1 | See attached catalogue for equipment detailed specification |
| FCU-C12 | 1 | Ceiling Casette Chilled Water Fan Coil Unit | Daikin/FWMJCC2BV1 | 1.5 | Private Room 8 | 230 | 60 | 1 | See attached catalogue for equipment detailed specification |
| FCU-C13 | 1 | Ceiling Casette Chilled Water Fan Coil Unit | Daikin/FWMJCC2BV1 | 2 | Treatment Room | 230 | 60 | 1 | See attached catalogue for equipment detailed specification |
| FCU-C14 | 1 | Ceiling Casette Chilled Water Fan Coil Unit | Daikin/FWMJCC2BV1 | 2.5 | 3- Bed Ward 2 | 230 | 60 | 1 | See attached catalogue for equipment detailed specification |
| FCU-C15 | 1 | Ceiling Casette Chilled Water Fan Coil Unit | Daikin/FWMJCC2BV1 | 1.5 | Private Room 9 | 230 | 60 | 1 | See attached catalogue for equipment detailed specification |
| FCU-C16 | 1 | Ceiling Casette Chilled Water Fan Coil Unit | Daikin/FWMJCC2BV1 | 1.5 | Private Room 10 | 230 | 60 | 1 | See attached catalogue for equipment detailed specification |
| FCU-C17 | 2 | Ceiling Casette Chilled Water Fan Coil Unit | Daikin/FWMJCC2BV1 | 3 | 5- BedWard 3 | 230 | 60 | 1 | See attached catalogue for equipment detailed specification |
| FCU-C18 | 2 | Ceiling Casette Chilled Water Fan Coil Unit | Daikin/FWMJCC2BV1 | 3 | 5- BedWard 4 | 230 | 60 | 1 | See attached catalogue for equipment detailed specification |
| FCU-C19 | 1 | Ceiling Casette Chilled Water Fan Coil Unit | Daikin/FWMJCC2BV1 | 1.5 | Private Room 10 | 230 | 60 | 1 | See attached catalogue for equipment detailed specification |
| FCU-C20 | 1 | Ceiling Casette Chilled Water Fan Coil Unit | Daikin/FWMJCC2BV1 | 1.5 | Private Room 11 | 230 | 60 | 1 | See attached catalogue for equipment detailed specification |
| FCU-C21 | 1 | Ceiling Casette Chilled Water Fan Coil Unit | Daikin/FWMJCC2BV1 | 1.5 | Private Room 12 | 230 | 60 | 1 | See attached catalogue for equipment detailed specification |
| FCU-C22 | 1 | Ceiling Casette Chilled Water Fan Coil Unit | Daikin/FWMJCC2BV1 | 1 | Private Room 13 | 230 | 60 | 1 | See attached catalogue for equipment detailed specification |
| FCU-C23 | 1 | Ceiling Casette Chilled Water Fan Coil Unit | Daikin/FWMJCC2BV1 | 1 | Private Room 14 | 230 | 60 | 1 | See attached catalogue for equipment detailed specification |
| FCU-C24 | 1 | Ceiling Casette Chilled Water Fan Coil Unit | Daikin/FWMJCC2BV1 | 1 | Private Room 15 | 230 | 60 | 1 | See attached catalogue for equipment detailed specification |
| FCU-C25 | 1 | Ceiling Casette Chilled Water Fan Coil Unit | Daikin/FWMJCC2BV1 | 1 | Private Room 16 | 230 | 60 | 1 | See attached catalogue for equipment detailed specification |
| FCU-C26 | 3 | Ceiling Casette Chilled Water Fan Coil Unit | Daikin/FWMJCC2BV1 | 2 | Waiting Area | 230 | 60 | 1 | See attached catalogue for equipment detailed specification |
| FCU-C27 | 1 | Ceiling Casette Chilled Water Fan Coil Unit | Daikin/FWMJCC2BV1 | 1 | Admitting | 230 | 60 | 1 | See attached catalogue for equipment detailed specification |
| FCU-C28 | 1 | Ceiling Casette Chilled Water Fan Coil Unit | Daikin/FWMJCC2BV1 | 1 | Billing | 230 | 60 | 1 | See attached catalogue for equipment detailed specification |
| FCU-C29 | 1 | Ceiling Casette Chilled Water Fan Coil Unit | Daikin/FWMJCC2BV1 | 1 | Cashier | 230 | 60 | 1 | See attached catalogue for equipment detailed specification |
| FCU-C30 | 2 | Ceiling Casette Chilled Water Fan Coil Unit | Daikin/FWMJCC2BV1 | 3.5 | Personel's Dining | 230 | 60 | 1 | See attached catalogue for equipment detailed specification |